For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the front seat head restraint. Refer to Front Seat Head Restraint Replacement .
3. Remove the front seat head restraint guides. Refer to Front Seat Head Restraint Guide Replacement .
4. Remove the front seat cushion outer trim panel. Refer to Front Seat Cushion Outer Trim Panel Replacement .
5. Remove the front seat cushion inner trim panel. Refer to Seat Cushion Inner Trim Panel Replacement .

1 | Seat Back Cushion Cover

#### Procedure

1. Disconnect the seat back cover j-channel.
2. Disconnect the seat back heater electrical connector, if equipped.
3. Remove the seat back cover and pad as an assembly from the seat back frame.
4. Separate the seat back cover from the seat back pad.

2 | Seat Back Cushion Pad