For 1990-2009 cars

Callout | Component Name
--- | ---

#### Rear Side Door Upper Hinge Assembly Replacement

1 | Rear Side Door Hinge Upper Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip: Replace only one hinge at a time. Tighten
35 N·m (26 lb ft)

2 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Rear Side Door Upper Hinge Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

#### Procedure

Check the door for proper alignment, adjust as necessary.

#### Rear Side Door Lower Hinge Assembly Replacement

4 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tip: Replace only one hinge at a time. Tighten 35 N·m (26 lb ft)
5 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
6 | Rear Side Door Lower Hinge Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

#### Procedure

Check the door for proper alignment, adjust as necessary.