For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system.
2. Remove the instrument panel (I/P) trim plates. Refer to the following procedures:

• | Instrument Panel Trim Panel Replacement - Right Side

• | Driver Information Display Switch Replacement

• | Instrument Panel Trim Panel Replacement - Left Side

• | Instrument Panel Outer Trim Cover Replacement

3. Remove the I/P cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
4. Remove the passenger inflatable restraint module. Refer to Inflatable Restraint Instrument Panel Module Replacement .
5. Remove the I/P upper trim pad air grille assembly. Refer to Defroster Grille Replacement .

1 | Instrument Panel Trim Pad Screw (Qty: 12) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.3 N·m (19 lb in)
2 | Instrument Panel Trim Pad Assembly

#### Procedure

1. Disconnect the electrical connections.
2. Lift up to release the I/P top panel from the I/P retainer.
3. When replacing trim pad assembly, transfer all necessary components.