For 1990-2009 cars

### Removal Procedure

1. Remove the starter. Refer to Starter Motor Replacement .
2. Disconnect the crankshaft position (CKP) sensor wiring harness electrical connector from the CKP sensor.
3. Remove the CKP sensor bolt.
4. Remove the CKP sensor.

### Installation Procedure

1. Lubricate the CKP sensor O-ring seal with clean engine oil.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CKP sensor.
3. Install the CKP sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Connect the CKP sensor wiring harness electrical connector to the CKP sensor.
5. Install the starter. Refer to Starter Motor Replacement .