For 1990-2009 cars

### Removal Procedure

1. Loosen the set screw in the base of the mirror.
2. Disconnect the electrical connector from the mirror, if equipped.
3. Remove the mirror from the mounting pad.

### Installation Procedure

1. Install the mirror to the mounting pad.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the mirror set screw.

Tighten
Tighten the set screw to 2 N·m (18 lb in).

3. Connect the electrical connector to the mirror, if equipped.