For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement

1 | Turn Signal Switch Bracket

#### Procedure

1. Release the plastic retaining tabs and remove the turn signal switch bracket from the steering column.
2. Disconnect any electrical connectors as needed, release the plastic retaining tabs, and remove the turn signal multifunction switch.
3. Disconnect any electrical connectors as needed, release the plastic retaining tabs, and remove the windshield wiper and washer switch.