For 1990-2009 cars

### Removal Procedure

1. Remove the cooling fan assembly from the vehicle. Refer to Cooling Fan and Shroud Replacement .
2. Scribe the position of each of the cooling fan blade on the cooling fan motor shaft.
3. Remove the cooling fan blade retaining clips and discard.
4. Remove the cooling fan blade.
5. Remove the cooling fan motor bolts and remove the cooling fan motor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the cooling fan motor and bolts.

Tighten
Tighten the bolts to 8 N·m (70 lb in).

2. Align the scribe marks on the cooling fan blade and motor shaft.
3. Install the cooling fan blade.
4. Install new retaining clips to the cooling fan blade.
5. Install the cooling fan assembly into the vehicle. Refer to Cooling Fan and Shroud Replacement .