For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the nut from the side window defog outlet grille.
3. Use a small, flat-bladed tool to release the tabs on the outlet grille. Remove the grille from the I/P top panel.

### Installation Procedure

1. Install the side window defog grille to the instrument panel (I/P) upper trim panel.

Important: Always use a new nut for the outlet grille.

2. Install a new nut to the outlet grille.
3. Check the outlet grille for proper fit and appearance.
4. Install the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .