For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the instrument panel cluster (IPC) trim. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .

1 | Cluster Assembly Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Cluster Assembly Tip Disconnect the electrical connector. Refer to Control Module References for programming and setup information.