For 1990-2009 cars

## Heater Outlet Hose Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the evaporator hose assembly. Refer to Air Conditioning Evaporator Hose Assembly Replacement
3. Remove the condenser tube. Refer to Condenser Tube Replacement

1 | Heater Outlet Hose

#### Procedure

Using J 38185 reposition the heater outlet hose clamps.

#### Special Tools

J 38185 Hose Clamp Pliers