For 1990-2009 cars

### Removal Procedure

1. Remove the console top cover. Refer to Front Floor Console Replacement.
2. Remove the shift cables from the shifter assembly. Refer to Shift Control Cable Replacement.
3. Remove the 2 front mounting nuts (2).
4. Remove the 2 rear mounting nuts (3) and the shifter.

### Installation Procedure

1. Position the shifter on the studs and install the front 2 nuts (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 rear nuts (3) and tighten to 25 N·m (18 lb ft).
3. Install the shift cables. Refer to Shift Control Cable Replacement.
4. Install the console. Refer to Front Floor Console Replacement.