For 1990-2009 cars

Caution: Refer to Brake Dust Caution in the Preface section.

1. Visually inspect the park brake lever and the lever pivot pin for the following conditions:

• | The lever being bent or broken at any point - particularly at the cable attachment

• | A seized or binding condition at lever pivot pin

• | A broken lever pivot pin

Important: The brake shoe and park brake lever are not serviced separately. If either component requires replacement, they must be replaced as an assembly.

2. If any of the conditions listed were found, the park brake lever and brake shoe assembly requires replacement.