For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seat back. Refer to Rear Split Folding Seat Back Replacement .
3. Remove the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement .

1 | Rear Seat Belt Anchor Bolt - Right Notice: Refer to Fastener Notice in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Rear Seat Belt Retractor Bolt- Right Tighten 45 N·m (33 lb ft)
3 | Rear Seat Belt Retractor Assembly- Right
4 | Rear Seat Belt Anchor Bolt- Center Tighten 45 N·m (33 lb ft)
5 | Rear Seat Belt Retractor Bolt - Center Tighten 45 N·m (33 lb ft)
6 | Rear Seat Belt Retractor Assembly- Center
7 | Rear Seat Belt Anchor Bolt- Left Tighten 45 N·m (33 lb ft)
8 | Rear Seat Belt Retractor Bolt- Left Tighten 45 N·m (33 lb ft)
9 | Rear Seat Belt Retractor Assembly- Left