For 1990-2009 cars

## Backup Lamp Replacement Pontiac G5

Callout | Component Name
--- | ---
1 | Back Up Lamp Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Back Up Lamp Assembly Tip Disconnect the electrical connector.

## Backup Lamp Replacement Chevrolet Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement .

1 | Back Up Lamp Nut (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Back Up Lamp Assembly

#### Procedure

1. Disconnect the electrical connector from the lamp socket.
2. Disengage the two lamp clips from the lamp pocket.
3. Push the lamp assembly outward, away from the rear compartment lid.
4. Replace or transfer the lamp socket and bulb as needed.