For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the cushion frame. Refer to Front Seat Cushion Frame Replacement .
3. Remove the seat back cover and pad assembly. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .

1 | Lumbar Actuator Screw (Qty: 2) Tighten 2 N·m (18 lb in)
2 | Lumbar Actuator