For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Bolt | 10 N·m | 89 lb in
Air Cleaner Intake Duct Bolt | 10 N·m | 89 lb in
Air Cleaner Nut | 10 N·m | 89 lb in
Air Cleaner Outlet Duct Clamp | 5 N·m | 44 lb in
Camshaft Position (CMP) Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Bolt | 10 N·m | 89 lb in
Evaporative Emission (EVAP) Canister Purge Valve Bracket Nut | 18 N·m | 13 lb ft
Exhaust Manifold Heat Shield Stud | 22 N·m | 16 lb ft
Fuel Fill Hose Clamp | 4.5 N·m | 40 lb in
Fuel Fill Pipe Bolt | 10 N·m | 89 lb in
Fuel Fill Pipe Lower Bolt | 10 N·m | 89 lb in
Fuel Filter Bracket Bolt | 10 N·m | 89 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 25 N·m | 18 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor (KS) | 25 N·m | 18 lb ft
Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Screw | 10 N·m | 89 lb in
Rear Brake Hose Bracket Nut | 10 N·m | 89 lb in
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in