For 1990-2009 cars

#### Special Tools

J 43482 Clutch Alignment Arbor

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement.
2. Remove the clutch cover bolts one turn at a time, until spring pressure is relieved.
3. Remove the clutch cover and the clutch disc.

### Installation Procedure

1. Install the clutch disc and the clutch cover.
2. Hand start the clutch cover to flywheel bolts, leaving the clutch cover loose enough to reposition for alignment.
3. Install the J 43482 in order to support the clutch cover to the flywheel assembly.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the clutch cover to flywheel bolts in the sequence shown to 30 N·m (22 lb ft).
5. Recheck each bolt torque using the tightening sequence.
6. Remove the J 43482 .
7. Install the transmission. Refer to Transmission Replacement.
8. Bleed the hydraulic system. Refer to Hydraulic Clutch Bleeding.
9. Connect the negative battery cable.