For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Odor originating or noticed through the HVAC system.
1 | Were you sent here from Symptoms or another diagnostic table? | Go to Step 2 | Go to Symptoms - HVAC Systems - Manual
2 |

1. Sit inside the vehicle.
2. Close all of the doors and windows.
3. Start the engine.
4. Allow the engine to idle at normal operating temperature.
5. Select the maximum blower speed.
6. Select the PANEL air outlet mode.
7. Select the coldest temperature setting.
8. Cycle through all of the blower speeds, modes, and temperatures to define what type of odor is present.

• | Musty smell

• | Coolant smell

• | Oil smell

Does the odor have a musty smell?

Go to Step 3

Go to Step 8

3 | Inspect the HVAC filter and the air inlet grille for debris. Is debris present? | Go to Step 4 | Go to Step 5
4 | Remove any debris. Is the action complete? | Go to Step 15 | --
5 | Inspect for wet carpeting. Is the carpet wet? | Go to Step 6 | Go to Step 8
6 | Inspect for the following conditions:

• | Water leaks around the windshield

• | Blockage of the HVAC module drain

• | Leaks around the door seals

Is a leak present?

Go to Step 7

Go to Step 15

7 | Repair the leak as necessary. Is the repair complete? | Go to Step 15 | --
8 | Does the odor have a coolant smell? | Go to Step 9 | Go to Step 12
9 | Inspect the cooling system for leaks. Refer to Loss of Coolant. Is a leak present? | Go to Step 10 | Go to Step 12
10 | Inspect for coolant leaking inside the vehicle or for a film build-up on the windshield. Is the condition present? | Go to Step 11 | Go to Step 15
11 | Replace the heater core. Refer to Heater Core Replacement. Is the repair complete? | Go to Step 15 | --
12 | Does the odor have an oily smell? | Go to Step 13 | Go to Step 15
13 |

1. Inspect the engine compartment for any leaks. Refer to the following procedures:

• | Oil Leak Diagnosis for the 2.0L engine

• | Oil Leak Diagnosis for the 2.2L or 2.4L engine

• | Fluid Leak Diagnosis for the 4T45-E transmission

2. Repair any oil leaks.

Is the repair complete?

Go to Step 15

--

14 | A musty odor can be caused by mold or mildew build-up on the evaporator or the heater core or inside of the HVAC module. Refer to Odor Correction. Is the action complete? | Go to Step 15 | --
15 | Operate the system in order to verify the repair. Did you find and correct the condition? | System OK | Go to Step 2