For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the charge air cooler outlet pipe. Refer to Intake Air Pressure and Temperature Sensor Replacement.

1 | Sensor Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Intake Air Pressure and Temperature Sensor

#### Procedure

Disconnect the electrical connector.