For 1990-2009 cars

1. Assemble the camshaft cover and gasket. Ensure that the gasket is located in the retaining groove in the camshaft cover.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the cover on the cylinder head and hand start the bolts.

Tighten
Tighten the camshaft cover bolts to 10 N·m (89 lb in).

3. Install the front lift bracket.

Tighten
Tighten the front lift bracket bolt to 25 N·m (18 lb ft).

4. Install the rear lift bracket.

Tighten
Tighten the rear lift bracket bolts to 25 N·m (18 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the ground strap.

Tighten
Tighten the camshaft cover ground strap bolts to 10 N·m (89 lb in).

6. Install the spark plugs.

Tighten
Tighten the spark plugs to 20 N·m (15 lb ft).

7. Install the ignition coil.
8. Install the ignition coil bolts.

Tighten
Tighten the ignition coil bolts to 10 N·m (89 lb in).