For 1990-2009 cars

Table 1: | Indicators
Table 2: | Driver Information Center

#### Indicators

Symbol | Reference
--- | ---
| ABS: ABS Description and Operation
| Air Bag: SIR System Description and Operation
(Export) BRAKE | Brake: Hydraulic Brake System Description and Operation
| Charge: Charging System Description and Operation
| Engine Coolant Temperature: Cooling System Description and Operation
| Engine Oil Pressure: The IPC illuminates the engine oil pressure (EOP) indicator when the PCM/ECM detects the EOP is low from the EOP switch.
| Front Fog Lamps: Exterior Lighting Systems Description and Operation
| High Beam: Exterior Lighting Systems Description and Operation
| MIL: Engine Control Module Description for the 2.2L engine, or Engine Control Module Description for the 2.4L engine
| Seatbelt: Seat Belt System Description and Operation
| Security: Content Theft Deterrent (CTD) Description and Operation
| Traction Disabled: ABS Description and Operation
| Turn Signals: Exterior Lighting Systems Description and Operation
| Upshift Indicator: The Upshift indicator notifies the driver when to shift to a higher transmission range. The IPC illuminates the Upshift indicator as determined by the PCM/ECM.

#### Driver Information Center

Message | Reference
--- | ---
AUTO LIGHTS OFF | Exterior Lighting Systems Description and Operation
AUTO LIGHTS ON | Exterior Lighting Systems Description and Operation
BATTERY SAVER ACTIVE | Charging System Description and Operation
BRAKE FLUID | Hydraulic Brake System Description and Operation
CHARGING SYSTEM ACTIVE | Charging System Description and Operation
CHANGE OIL SOON | The DIC displays this message when the PCM/ECM determines that the engine oil life is less than a pre-determined value. Refer to GM Oil Life System Resetting
CHECK GAS CAP | Evaporative Emission Control System Description for the 2.0L engine, Evaporative Emission Control System Description for the 2.2L engine or Evaporative Emission Control System Description for the 2.4L engine
CRUISE CONTROL ACTIVE | Cruise Control Description and Operation
DOOR AJAR | Power Door Locks Description and Operation
ENG PWR REDUCED | Cooling System Description and Operation
ICE POSSIBLE | The driver information center (DIC) displays this message when the outside air temperature drops below 2°C (36°F). When the temperature rises above 5.5°C (42°F), the message turns OFF.
KEY FOB BATT LOW | Keyless Entry System Description and Operation
LOW COOLANT | Cooling System Description and Operation
LOW FUEL | The DIC displays this message when the ECM/PCM detects that the fuel level is below a pre-determined value from the fuel level sensor.
LOW OIL LEVEL | The DIC displays this message when the PCM/ECM detects a low oil level condition.
LOW WASHER FLUID | Wiper/Washer System Description and Operation
LOW TRACTION | ABS Description and Operation
POWER STEERING | Power Steering System Description and Operation
PARKING BRAKE | Park Brake System Description and Operation
SERVICE AIR BAG | SIR System Description and Operation
SERVICE VEHICLE SOON | The driver information center (DIC) displays this message when the BCM or ECM/PCM detects certain vehicle malfunctions that are not emissions related.
STARTING DISABLED | Starting System Description and Operation
TRUNK AJAR | Luggage Compartment Description and Operation