For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the wheel. Refer to Tire and Wheel Removal and Installation .
3. Support the rear axle with a tall jack stand near the shock absorber.
4. Remove the upper and lower shock bolts.
5. Remove the shock from the vehicle.

### Installation Procedure

1. Position the shock absorber to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install NEW upper and lower shock bolts.

Tighten

• | Tighten the upper bolt to 90 N·m (66 lb ft).

• | Tighten the lower bolt to 110 N·m (81 lb ft).

3. Remove the jack stand.
4. Install the wheel. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.