For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief.
2. Remove the right rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Plastic Tie Strap (Qty: 3)

#### Procedure

Cut the plastic tie straps and replace with new tie straps.

2 | Evaporative Emission (EVAP) Canister Connector

#### Procedure

Disconnect the connector. Refer to Plastic Collar Quick Connect Fitting Service.

3 | EVAP Canister Vent Rear Pipe

#### Procedure

Pull down while twisting toward the rear of the vehicle.