For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Wastegate Actuator Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Disconnect the vacuum hose.

Tighten
10 N·m (89 lb in)

2 | Turbocharger Wastegate Actuator