For 1990-2009 cars

#### Special Tools

J 41545 Park/Neutral Switch Aligner

### Adjustment

1. Disconnect the transaxle range switch electrical connectors from the switch.
2. Remove the shift control cable from the transaxle range switch lever.
3. Remove the transaxle range switch lever and nut
4. Make sure the transaxle manual shaft is in the Neutral position.
5. Loosen, DO NOT REMOVE the transaxle range switch bolts.
6. Insert the J 41545 as shown and rotate the switch until the tool drops onto position.

Caution: Refer to Fastener Caution in the Preface section.

7. Tighten the transaxle range switch bolts to 20 N·m (15 lb ft).
8. Remove the alignment tool.

Note: After adjusting the switch, verify the engine only starts in Park or Neutral. If the engine starts in any other position, adjust the switch.

9. Install the transaxle range switch lever and nut and tighten to 35 N·m (26 lb ft)
10. Connect the transaxle range switch electrical connectors to the switch.
11. Install the shift control cable to transaxle range switch lever and verify proper operation.