For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering wheel. Refer to Steering Wheel Replacement.
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement.

1 | Ignition Lock Cylinder Solenoid Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Ignition Lock Cylinder Solenoid

#### Procedure

Disconnect any electrical connectors as needed.

Tip
A new ignition lock cylinder solenoid consists of only the solenoid and spring. Do not attempt to remove any roll pins retaining the plunger mechanism. If the plunger mechanism exhibits any signs of damage or wear then replacement of the ignition lock cylinder case will be necessary.