For 1990-2009 cars

## Rear License Plate Lamp Replacement Chevrolet

### Removal Procedure

1. Remove the license plate from the rear bumper fascia.
2. Remove the screws (1) from the license plate lamp.
3. Remove the license plate lamp (2) from the rear bumper fascia.
4. Remove the bulb/socket from the license plate lamp (2) by turning counterclockwise.
5. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Install the socket to the license plate lamp (2) by turning the socket clockwise.
3. Install the license plate lamp (2) to the rear bumper fascia.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the screws (1) to the license plate lamp. Tighten the license plate lamp screws to 2 N·m (18 lb in).
5. Install the license plate to the rear bumper fascia.

## Rear License Plate Lamp Replacement Pontiac G5

Callout | Component Name
--- | ---
1 | License Plate Lamp Assembly Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | License Plate Lamp Assembly Tip Remove the lamp assembly from inside the rear bumper fascia and disconnect the bulb socket.