For 1990-2009 cars

### Removal Procedure

1. Remove the shift control knob. Refer to Transmission Control Lever Knob Replacement .
2. Pry up on the shift control boot trim from the front of the shift control boot assembly.
3. Remove the shift control boot.

### Installation Procedure

1. Install the shift control boot to the vehicle.
2. Install the shift control boot trim to the console assembly.
3. Install the shift control knob. Refer to Transmission Control Lever Knob Replacement .