For 1990-2009 cars

1. Assemble the camshaft cover and gasket. Ensure that the gasket is located in the retaining groove in the camshaft cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cover on the cylinder head and hand start the bolts.

Tighten
Tighten the camshaft cover bolts to 10 N·m (89 lb in).

3. Install the front lift bracket.
4. Install the front lift bracket bolt.

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

5. Install the rear lift bracket.
6. Install the rear lift bracket bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

7. Install the ground strap.

Tighten
Tighten the camshaft cover ground strap bolts to 10 N·m (89 lb in).

8. Install the spark plugs.

Tighten
Tighten the spark plugs to 20 N·m (15 lb ft).

9. Install the ignition coil.

Tighten
Tighten the ignition coil bolts to 10 N·m (89 lb in).

10. Install the camshaft position actuator solenoid valves.
11. Install the camshaft position actuator solenoid valve bolts.