For 1990-2009 cars

### Removal Procedure

1. Remove the clutch pedal position switch (2) from the clutch pedal .
2. Remove the electrical connector (1) from the clutch pedal position switch (2).

### Installation Procedure

1. Install the electrical connector (1) to the clutch pedal position switch (2).
2. Install the clutch pedal position switch to the clutch pedal.
3. Push the clutch pedal all the way to the floor to adjust the switch.