For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section.

#### Preliminary Procedures

1. Remove the steering column opening filler assembly. Refer to Steering Column Opening Filler Replacement.
2. Tilt the steering wheel up.

1 | Electronic Traction Control Switch Clip (Qty: 2)
2 | Electronic Traction Control Switch Assembly

#### Procedure

1. Release the switch assembly by pulling away from the instrument panel retainer.
2. Disconnect the electrical connector.