For 1990-2009 cars

#### Tools Required

• | J 39400-A Halogen Leak Detector

• | J 46246 Valve Core Tool

### Removal Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the service port valve core using J 46246 or equivalent.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the service port valve core using J 46246 or equivalent.

Tighten
Tighten the service port valve core to 2.5 N·m (22 lb in).

2. Evacuate and charge the refrigerant system. Refer to Refrigerant Recovery and Recharging .
3. Leak test the fittings using the J 39400-A .