For 1990-2009 cars

### Removal Procedure

1. Remove the underhood electrical center bracket from the vehicle and reposition the electrical center. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
2. Support the transmission with a floor jack. Use a piece of wood between the jack and the transmission.
3. Remove the transmission mount-to-transmission bracket bolts.
4. Remove the transmission mount to mid-rail bolts.
5. Using a floor jack, slowly lower the transmission enough to remove the transmission mount from the vehicle.

### Installation Procedure

1. Install the transmission mount to the mid-rail.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transmission mount to mid-rail bolts.

Tighten
Tighten the bolts to 27 N·m (20 lb ft).

3. Using a floor jack, raise the transmission until it contacts the transmission mount.

Important: The transmission mount to transmission bolts must be hand started. Do not pry the transmission or mount to align the holes.

4. Hand start the transmission mount to bracket bolts using the following sequence:

4.1. | Rear bolt

4.2. | Middle bolt

4.3. | Front bolt

5. Using the previous sequence, tighten the transmission mount bolts.

Tighten
Tighten the bolts to 65 N·m (48 lb ft).

6. Install the underhood electrical center bracket to the vehicle and install the electrical center into position on the bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .