For 1990-2009 cars

## Engine Coolant Thermostat Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Disconnect the radiator surge tank outlet hose/pipe. Refer to Radiator Surge Tank Outlet Hose/Pipe Replacement.
3. Disconnect the radiator outlet hose from the water inlet assembly. Refer to Radiator Outlet Hose Replacement.

1 | Water Inlet Assembly Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Water Inlet Assembly
3 | Engine Coolant Thermostat