For 1990-2009 cars

## Center Pillar Lower Garnish Molding Replacement Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the center pillar upper garnish. Refer to Center Pillar Upper Garnish Molding Replacement .
2. Remove the front carpet retainer. Refer to Front Carpet Retainer Replacement .
3. Remove the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .
4. Position the seat in the full forward position.

1 | Center Pillar Lower Panel Assembly
2 | Panel Assembly Center Pillar Lower Retainer