For 1990-2009 cars

## Rear Side Marker Lamp Replacement Pontiac G5

Callout | Component Name
--- | ---
1 | Rear Side Marker Lamp Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Side Marker Lamp Housing

#### Procedure

1. Pull the rearward edge of the lamp away from the rear bumper fascia in order to release the front tab.
2. Rotate the electrical bulb socket harness counter-clockwise and remove from the lamp housing.