For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket.
2. Remove the seat cushion inner trim panel. Refer to Seat Cushion Inner Trim Panel Replacement.
3. Remove the seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement.

1 | Seat Belt Buckle Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Seat Belt Buckle Assembly