For 1990-2009 cars

Warning: Refer to Brake Dust Warning in the Preface section.

### Removal Procedure

Caution: Support the brake caliper with heavy mechanic wire, or equivalent, whenever it is separated from its mount and the hydraulic flexible brake hose is still connected. Failure to support the caliper in this manner will cause the flexible brake hose to bear the weight of the caliper, which may cause damage to the brake hose and in turn may cause a brake fluid leak.

1. Remove the brake caliper from the brake caliper mounting bracket and support the brake caliper with heavy mechanic's wire, or equivalent. Do NOT disconnect the hydraulic brake flexible hose from the caliper. Refer to Rear Brake Caliper Replacement.
2. Remove the brake pads from the brake caliper bracket.
3. Remove the brake pad retainers (1) from the brake caliper bracket.
4. If reusing the bracket, thoroughly clean the pad hardware mating surfaces of the caliper bracket (2), of any debris and corrosion.
5. Inspect the disc brake pad retainers (1) for the following:

• | Bent mounting tabs

• | Excessive corrosion

• | Looseness at the brake caliper mounting bracket

• | Looseness at the disc brake pads

6. If any of the conditions listed are found, the disc brake pad retainers require replacement.
7. Remove the brake caliper mounting bracket bolts (1).
8. Remove the brake caliper bracket from the rear axle.
9. Inspect the caliper bracket. If the brake caliper bracket is bent, cracked, or damaged, it requires replacement.
10. Inspect the brake caliper guide pins (1, 4) for freedom of movement, and inspect the condition of the guide pin boots (2). Move the guide pins inboard and outboard within the bracket bores, without disengaging the slides from the boots, and observe for the following:

• | Restricted caliper guide pin movement

• | Looseness in the brake caliper mounting bracket

• | Seized or binding caliper guide pins

• | Split or torn boots

11. If any of the conditions listed are found, the brake caliper guide pins and/or boots require replacement.

### Installation Procedure

1. Install the brake caliper mounting bracket to the rear axle.

Caution: Refer to Fastener Caution in the Preface section.

Notice: This is a self-retaining fastener joint that does not require thread locking compounds. Do not attempt to clean the threads with a standard tap. If a standard tap is used, damage to the joint threads will occur.

2. Install the brake caliper mounting bracket bolts (1).

Tighten
Tighten the bolts to 115 N·m (85 lb ft).

3. Apply a very thin coating of high temperature silicone brake lubricant to the pad hardware mating surfaces of the caliper bracket (2) only.
4. Clean the brake pad mating surfaces of the brake pad retainers (1).
5. Install the brake pad retainers (1) to the brake caliper bracket.

Note: The wear sensor equipped disc brake pad must be mounted inboard of the rotor with the leading edge of the sensor facing the brake rotor during forward wheel rotation, or at the bottom of the pad when installed in vehicle position.

6. Install the brake pads to the brake caliper bracket.
7. Remove the support and reposition the brake caliper over the brake pads and to the mounting bracket. Refer to Rear Brake Caliper Replacement.