For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the steering wheel. Refer to Steering Wheel Replacement
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement.

1 | Inflatable Restraint Steering Wheel Module Coil Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Inflatable Restraint Steering Wheel Module Coil

#### Procedure

1. Disconnect any electrical connectors as needed.
2. If re-centering of the inflatable restraint steering wheel module coil is needed then refer to Inflatable Restraint Steering Wheel Module Coil Centering.