For 1990-2009 cars

#### Tools Required

J 42067 Rear Main Seal Installer

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement .
2. Remove the flywheel.

Important: Do not damage the outside diameter of the crankshaft or chamber with any tool.

3. Pry the crankshaft rear oil seal with a flat-bladed tool.

### Installation Procedure

1. Use the J 42067 and install the seal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the flywheel.

Tighten
Tighten the flywheel bolts to 53 N·m (39 lb ft) plus 25 degrees.

3. Install the transmission. Refer to Transmission Replacement .