For 1990-2009 cars

# Steering Column Shudder, Noise, Vibration While Making Right Hand Turns at 5-15 MPH (8-24 KM/H) (Pull Fuse)

Subject: | Steering Column Shudder, Noise, Vibration While Making Right Hand Turns at 5-15 MPH (8-24 KM/H) (No Fix Available At This Time)

Models: | 2005-2007 Chevrolet Cobalt

| 2005-2006 Pontiac Pursuit (Canada Only)

| 2007 Pontiac G5

This bulletin is being revised to provide additional diagnostic information. Please discard Corporate Bulletin Number 06-02-35-008A (Section 02 -- Steering).

### Condition

Some customers may comment on a shudder, noise or vibration that is felt through the steering column while making right hand turns at 5-15 mph (8-24 km/h). This condition can be duplicated by the technician. Removal of the 60 amp fuse that powers the EPS may eliminate the condition.

### Correction

DO NOT REPLACE THE STEERING COLUMN.

Replacement of the steering column, P/N 10394224, is NOT recommended. Steering column replacement has been proven to be ineffective in several Technical Assistance cases.

Pull the 60 amp steering fuse (1) in the underhood fuse block. If this eliminates the shudder/vibration concern, contact Technical Assistance for further information in order to repair the vehicle. If this does not eliminate the shudder/vibration, continue to diagnose the vehicle according to the diagnostics in SI.