For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Control Arm Nut and Bolts | 68 N·m | 50 lb ft
Ball Joint to Steering Knuckle Nut

- First Pass

50 N·m

Reverse Nut 3/4 turn

37 lb ft

Reverse Nut 3/4 turn

- Second Pass

50 N·m + 30°

37 lb ft +30°

Control Arm to Front Frame Bolts | 55 N·m | 41 lb ft
Control Arm to Rear Frame Bolts | 100 N·m + 180° | 74 lb ft +180°
Frame to Chassis Bolts | 100 N·m + 180° | 74 lb ft +180°
Intermediate Shaft Pinch Bolt | 34 N·m | 25 lb ft
Stabilizer Link to Strut Nut | 65 N·m | 48 lb ft
Stabilizer Shaft Clamp Bolt | 50 N·m | 37 lb ft
Stabilizer Shaft Link to Stabilizer Bar Nut | 80 N·m | 59 lb ft
Strut Assembly to Steering Knuckle Nut | 120 N·m | 89 lb ft
Strut to Body Nut | 20 N·m | 15 lb ft
Strut Shaft Nut | 70 N·m | 52 lb ft
Transmission Mount Through Bolt | 100 N·m | 74 lb ft
Transmission Mount to Frame Bolt | 50 N·m | 37 lb ft
Wheel Bearing/Hub Assembly Mounting Bolts | 115 N·m | 85 lb ft