For 1990-2009 cars

### Removal Procedure

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

1. Drain the fuel tank. Refer to Fuel Tank Draining .
2. Remove the fuel fill pipe to fill pipe housing bolts.
3. Remove the fuel fill pocket. Refer to Fuel Tank Filler Pipe Housing Replacement .
4. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
5. Remove the fuel fill pipe lower bolt.
6. Disconnect the fuel tank vent pipe quick connect fittings (1, 3). Refer to Plastic Collar Quick Connect Fitting Service .
7. Loosen the fuel fill pipe hose clamp (2) at the fuel tank.
8. Remove the fuel fill pipe hose from the fuel tank.
9. Remove the fuel fill pipe from the vehicle.

### Installation Procedure

1. Install the fuel fill pipe to the vehicle.
2. Install the fuel fill pipe hose to the fuel tank.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the fuel fill pipe hose clamp (2) at the fuel tank.

Tighten
Tighten the clamp to 4.5 N·m (40 lb in).

4. Connect the fuel tank vent pipe quick connect fittings (1, 3). Refer to Plastic Collar Quick Connect Fitting Service .
5. Instal the fuel fill pipe lower bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

6. Lower the vehicle.
7. Install the fuel fill pocket. Refer to Fuel Tank Filler Pipe Housing Replacement .
8. Install the fuel fill pipe to fill pipe housing bolts.

Tighten
Tighten the bolts to 1.5 N·m (13 lb in).

9. Refill the fuel tank.
10. Install the fuel fill cap.