For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement.
2. Disconnect the exhaust camshaft position (CMP) sensor electrical connector (1).
3. Remove the CMP sensor bolt. Intake CMP shown, exhaust CMP similar.
4. Remove the CMP sensor.

### Installation Procedure

Note: Inspect the CMP sensor for damage, replace as necessary.

1. Lubricate the CMP sensor O-ring seal with clean engine oil.
2. Install the CMP sensor. Intake CMP shown, exhaust CMP similar.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the CMP sensor bolt and tighten to 10 N·m (89 lb in).
4. Connect the exhaust CMP sensor electrical connector (1).
5. Install the intake manifold cover. Refer to Intake Manifold Cover Replacement.