For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the armrest pull cup. Refer to Armrest Pull Cup Replacement.
2. Remove the manual window regulator handle if equipped. Refer to Door Window Regulator Handle Replacement.
3. Disconnect the inside door handle cable. Refer to Door Inside Handle Replacement.

1 | Side Door Trim Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.2 N·m (19 lb in)
2 | Side Door Trim Panel Assembly
3 | Side Door Trim Retainer