For 1990-2009 cars

### Removal Procedure

1. Remove the console top cover. Refer to Front Floor Console Replacement.
2. Remove the shift cables from the shifter assembly. Refer to Shift Control Cable Replacement .
3. Remove the 2 front mounting nuts (2).
4. Remove the 2 rear mounting nuts (3) and the shifter.

### Installation Procedure

1. Position the shifter on the studs and install the front 2 nuts (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 2 rear nuts (3).

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

3. Install the shift cables. Refer to Shift Control Cable Replacement .
4. Install the console. Refer to Front Floor Console Replacement.