For 1990-2009 cars

### Removal Procedure

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

1. Drain the fuel tank. Refer to Fuel Tank Draining .
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Loosen the fuel filler hose clamps (1, 2).
4. Disconnect the fuel filler hose from the fuel tank.
5. Disconnect the fuel filler hose from the fuel filler pipe.

### Installation Procedure

1. Connect the fuel filler hose to the fuel filler pipe.
2. Connect the fuel filler hose to the fuel tank.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the fuel filler hose clamps (1, 2).

Tighten
Tighten the clamps to 4.5 N·m (40 lb in).

4. Lower the vehicle.
5. Refill the fuel tank.