For 1990-2009 cars

### Removal Procedure

1. Move the wiper arm to the service up position
2. Press the wiper blade clip button in to release the wiper blade from the inside radius of the wiper arm.
3. Remove the wiper blade out through the opening in the wiper arm.

### Installation Procedure

1. Install the hook of the wiper arm through the opening in the wiper blade.
2. Press the wiper blade pivot into the wiper arm hook until the pivot locks into the hook.
3. Position the wiper blade pivot in the inside radius of the wiper arm hook.
4. Move the wiper arm back to the parked position.
5. Operate the windshield wipers and inspect for proper operation.