For 1990-2009 cars

## Parking Brake Rear Cable Replacement Disc

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Ensure that the park brake lever is in the fully released position.
3. Release the tension from the park brake cables.

Using ONLY HAND TOOLS, loosen the adjusting nut (1) completely to the end of the front cable threaded rod.

4. Remove the rear seat lower cushion. Refer to Rear Seat Cushion Replacement.
5. Remove the rear carpet retainers. Refer to Rear Carpet Retainer Replacement .
6. Position the carpet forward in order to access the rear park brake cables and body pass-thru grommets.
7. With the park brake lever in the released position, release the appropriate rear park brake cable end (3) from the cable equalizer.
8. Release the rear cable fitting (2) from the park brake lever bracket (1) and remove the cable from the lever assembly.
9. Release the rear park brake cable body pass-thru grommet.
10. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
11. If the park brake cable is being reused, release the tab on the underbody retainer (2) and remove the park brake cable from the retainer.
12. If a new park brake cable will be installed, release the underbody retainer (2) from the vehicle underbody.

Important: Do NOT pull on the park brake cable to release the C-shaped retainer (1) on the cable from the bracket at the rear axle trailing arm pivot.

13. Using a suitable tool, carefully pry against the edge of the C-shaped retainer (1) on the park brake cable, to release the retainer from the bracket at the rear axle trailing arm pivot.
14. Remove the cable from the opening in the vehicle underbody.
15. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
16. Release the park brake cable end (1) from the caliper park brake lever.
17. Using a flat-bladed screwdriver, depress the retaining tabs (4) on the park brake cable fitting, and release the cable fitting from the cable bracket.
18. Remove the park brake cable guide (3) retaining bolt (2), and remove the cable.

### Installation Procedure

1. Insert the park brake cable through the cable bracket on the caliper.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear park brake cable guide (3) retaining bolt (2).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Secure the cable fitting to the cable bracket. Ensure that the retaining tabs (4) are fully seated.
4. Install the cable end (1) to the caliper park brake lever.
5. Install the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
6. Insert the cable through the opening in the vehicle underbody.
7. Install the C-shaped retainer (1) on the park brake cable into the bracket at the rear axle trailing arm pivot.
8. Install and secure park brake cable pass-thru grommet (3) to the opening in the vehicle underbody.
9. If a new park brake cable is being installed, secure the underbody retainer (2) to the vehicle underbody.
10. If the park brake cable is being reused, install the park brake cable to the underbody retainer (2) and press the tab into place to secure.
11. Lower the vehicle.
12. Secure the cable fitting (2) to the park brake lever bracket (1). Attempt to pull the park brake cable free of the lever bracket, to ensure that the retaining tabs on the fitting are properly secured.
13. Install the cable end (3) to the cable equalizer.
14. Reposition the carpet to the installed position.
15. Install the rear carpet retainers. Refer to Rear Carpet Retainer Replacement .
16. Install the rear seat lower cushion. Refer to Rear Seat Cushion Replacement .
17. Adjust the park brake cable tension. Refer to Park Brake Adjustment .
18. Install the front floor console. Refer to Front Floor Console Replacement .

## Parking Brake Rear Cable Replacement Drum

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Ensure that the park brake lever is in the fully released position.
3. Release the tension from the park brake cables.

Using ONLY HAND TOOLS, loosen the adjusting nut (1) completely to the end of the front cable threaded rod.

4. Remove the rear seat lower cushion. Refer to Rear Seat Cushion Replacement .
5. Remove the rear carpet retainers. Refer to Rear Carpet Retainer Replacement .
6. Position the carpet forward in order to access the rear park brake cables and body pass-thru grommets.
7. With the park brake lever in the released position, release the appropriate rear park brake cable end (3) from the cable equalizer.
8. Release the rear cable fitting (2) from the park brake lever bracket (1) and remove the cable from the lever assembly.
9. Release the rear park brake cable body pass-thru grommet.
10. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
11. If the park brake cable is being reused, release the tab on the underbody retainer (2) and remove the park brake cable from the retainer.
12. If a new park brake cable will be installed, release the underbody retainer (2) from the vehicle underbody.

Important: Do NOT pull on the park brake cable to release the C-shaped retainer (1) on the cable from the bracket at the rear axle trailing arm pivot.

13. Using a suitable tool, carefully pry against the edge of the C-shaped retainer (1) on the park brake cable, to release the retainer from the bracket at the rear axle trailing arm pivot.
14. Remove the cable from the opening in the vehicle underbody.
15. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
16. Remove the brake drum. Refer to Brake Drum Replacement .
17. Using a flat-bladed screwdriver, depress the visible retaining tab (1) on the park brake cable fitting, then tilt the released side of the cable end back into the backing plate.
18. Rotate the park brake cable to expose the other retaining tab.
19. Using a flat-bladed screwdriver, depress the remaining retaining tab on the park brake cable fitting, and release the cable fitting from the backing plate.
20. Move the majority of the cable return spring back through the opening in the backing plate.
21. Push the cable toward the rear of the vehicle, just enough to clear the cable end from the slot on the park brake lever.
22. Using a flat-bladed screwdriver, lift the cable to fully release the cable from the lever, then remove the cable.

### Installation Procedure

1. Insert the park brake cable through the opening in the backing plate. Only install the cable return spring to just rearward of the spring positioning tab on the backing plate.
2. Push the cable toward the rear of the vehicle, along the outside of the trailing brake shoe, until the cable end is positioned just past the slot on the park brake lever.
3. While holding the cable in position from front to rear, move the cable end to the back of the park brake lever.
4. Press the cable down into the slot on the lever, then pull the cable toward the front of the vehicle to secure the cable end to the slot.
5. While continuing to pull the cable away from the lever, insert a flat-bladed screwdriver into the opening on the lever to prevent the cable from lifting out of the slot on the lever.
6. Move the cable return spring through the opening in the backing plate.
7. Secure the cable fitting to the backing plate. Attempt to pull the park brake cable free of the backing plate, to ensure that the retaining tabs (1) on the fitting are properly secured.
8. Adjust the rear drum brakes. Refer to Drum Brake Adjustment .
9. Install the brake drum. Refer to Brake Drum Replacement .
10. Install the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
11. Insert the cable through the opening in the vehicle underbody.
12. Install the C-shaped retainer (1) on the park brake cable into the bracket at the rear axle trailing arm pivot.
13. Install and secure park brake cable pass-thru grommet (1) to the opening in the vehicle underbody.
14. If a new park brake cable is being installed, secure the underbody retainer (2) to the vehicle underbody.
15. If the park brake cable is being reused, install the park brake cable to the underbody retainer (2) and press the tab into place to secure.
16. Lower the vehicle.
17. Secure the cable fitting (2) to the park brake lever bracket (1). Attempt to pull the park brake cable free of the lever bracket, to ensure that the retaining tabs on the fitting are properly secured.
18. Install the cable end (3) to the cable equalizer.
19. Reposition the carpet to the installed position.
20. Install the rear carpet retainers. Refer to Rear Carpet Retainer Replacement.
21. Install the rear seat lower cushion. Refer to Rear Seat Cushion Replacement .
22. Adjust the park brake cable tension. Refer to Park Brake Adjustment .
23. Install the front floor console. Refer to Front Floor Console Replacement.