For 1990-2009 cars

## Radiator Outlet Hose Replacement 2.0L (LSJ)

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Lower the vehicle.
3. Remove the air intake duct.
4. Remove the fan shroud. Refer to Fan Shroud Replacement .
5. Reposition the radiator outlet hose clamp at the radiator using J 38185 .
6. Remove the radiator outlet hose from the radiator.
7. Remove the underhood electrical center. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
8. Reposition the radiator outlet hose clamp at the engine using J 38185 .
9. Remove the radiator outlet hose from the engine.

### Installation Procedure

1. Install the radiator outlet hose to the radiator.
2. Reposition the radiator outlet hose clamp to secure the hose using J 38185 .
3. Install the underhood electrical center. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
4. Install the radiator outlet hose to the engine.
5. Reposition the radiator outlet hose clamp to secure the hose using J 38185 .
6. Install the fan shroud. Refer to Fan Shroud Replacement .
7. Install the air intake duct.
8. Fill the cooling system. Refer to Cooling System Draining and Filling .

## Radiator Outlet Hose Replacement 2.2L (L61), 2.4L (LE5)

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling .

1 | Radiator Outlet Hose Assembly Tip

• | Using J 38185 , position the radiator outlet hose clamps aside and remove the hose from the fittings.

• | Note routing of the radiator outlet hose to ensure proper installation.